ANEXO CIRCULAR 2 Y51954

RESPUESTA Nro. 3

|  |  |  |  |
| --- | --- | --- | --- |
| Switch Name | Dom | World Wide Name | Model Spd  (Switch Speed)  OSVer  (Operating System Version) Status DaysUp Pwr(W) (Power used, in watts.) Mode Serial Number Ports(Total ports including ICLs) Unused   (Unused Ports) Unlicnsd   (Unlicensed Ports) |
| swpar09\_6520 | 22 | 10:00:50:eb:1a:e8:5c:48 | 652016G 7.4.1b Healthy 769 99 Native   CHQ2542L022     (OEM Serial Number: USB542D00D) 96 (96) 4 48 |
| swag08\_8510 | 31 | 10:00:50:eb:1a:c6:5e:9c | DCX-8510-416G 7.4.1b Healthy 581 1026 Native   ANN2541L00F     (OEM Serial Number: USB541B00F)(Chassis Serial Number: ANP3023L04P) 96 (160) 79 0 |
| swag09\_6520 | 32 | 10:00:50:eb:1a:e8:56:40 | 652016G 7.4.1b Healthy 581 99 Native   CHQ2542L026     (OEM Serial Number: USB542D00H) 96 (96) 13 48 |

|  |  |  |
| --- | --- | --- |
| Switch Name | Dom  (Switch Domain) | World Wide NameModel  Spd  (Switch Speed)  OSVer  (Operating System Version) Status DaysUp Pwr(W) (Power used, in watts.) Serial Number Ports (Total ports including ICLs) Unusd  Ports UnLicnd  (Unlicensed Ports) |
| swag10\_6520 | 11 | 10:00:50:eb:1a:e8:42:b86520 16G 7.4.1b Healthy 32 99 CHQ2542L01Z   (OEM Serial Number: USB542D00A) 96 (96) 12 48 |